{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["mo-3.2 Pre-Fligh Check (E)"],"not_rendered":{"images":1},"read":"whole","date_system":"1900"}

{"sheet":"mo-3.2 Pre-Fligh Check (E)","index":0,"n_rows":16,"n_cols":9,"rows_kept":16,"merged":[[0,0,0,9],[1,0,1,9],[2,1,2,2],[2,4,2,5],[2,7,2,9],[3,1,3,7],[4,0,4,9],[5,1,5,2],[5,3,5,4],[6,1,6,9],[7,0,7,9],[9,0,9,9],[12,0,12,9],[15,6,15,8]]}
["Drone Management Group                                                                                                                                                             Emergency Mission - Pre-Flight Inspection Check List mo-3.2 (E)"]
["Pilot and Organization Information"]
["Pilot Name",null,null,"Organization",null,null,"Visual Observer Name"]
["Location Address",{"$nulls":7},"Date"]
["Airspace Assessment"]
["Type of Airspace",null,null,"Weather Minimums Satisfied",null,null,"TFR",null,"NOTAM Filed"]
["Airspace Notes"]
["Site / Location Assessment"]
["Secure Perimeter",null,"Secure TOLZ",null,"Identify Obstructions",null,"Signal Interference",null,"Signal Strength"]
["Controller Inspection"]
["Controller Functioning ",null,"Antennas",null,"Batteries",null,"GPS",null,"IMU"]
["Compass",null,"Update Firmware",null,"Obstacle Avoidance",null,"Set Home Point",null,"Return to Home Altitude"]
["Aircraft Inspection"]
["UAV Airframe ",null,"Motors",null,"Props",null,"Batteries",null,"Landing Gear"]
["Lighting",null,"Gimbles (locks)",null,"Sensors        (lens cap)",null,"SD Card",null,"Recording On"]
["External Payload",null,"Verify Telemetry",null,"Verify Link",null,"Flight Control Check When Airborne"]